(footprint "7427932" (version 20201220) (generator pcbnew) (layer "F.Cu")
  (tedit 600D90A9)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c95a082-0a24-4a02-b3f0-aedc0e528d46)
  )
  (fp_text value "7427932" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 67ce961c-e568-4ff5-a4c3-aef24e71253e)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d38fd966-d107-4270-85f5-986b2d4500b1)
  )
  (fp_line (start -3.6 -2.4) (end 3.5 -2.4) (layer "F.SilkS") (width 0.12) (tstamp 1ba37db9-6d39-4dec-8e19-6fa1beef5abd))
  (fp_line (start -3.6 2.4) (end 3.5 2.4) (layer "F.SilkS") (width 0.12) (tstamp 4ebc86cf-d49c-452b-bdac-3b33d2e13332))
  (fp_rect (start 4.4 2.4) (end -4.4 -2.4) (layer "F.Fab") (width 0.12) (fill none) (tstamp ee609834-7e7e-4fe9-9fae-811014c126bb))
  (pad "1" smd rect (at -3.65 0) (size 3 1.47) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c6cfe893-816c-4f28-bf88-fb534282273d))
  (pad "2" smd rect (at 3.65 0) (size 3 1.47) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8ae7a6f1-ce42-456a-b9ca-ab35584e7878))
  (model "${KIPRJMOD}/3D/7427932 (rev1).stp"
    (offset (xyz 0 0 1.7))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 0))
  )
)
